;; Realtek 10/100/1000 PCI-E NIC Family all in one NDIS Driver
;;
;; Copyright 2008, Realtek Semiconductor Corporation.
;;
;; This product is covered by one or more of the following patents:
;; US5,307,459, US5,434,872, US5,732,094, US6,570,884, US6,115,776, 
;; and US6,327,625.
;;
;; This release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT = netrtle.cat                        ;;for WHQL certified
DriverVer      = 10/30/2008,5.708.1030.2008

[Manufacturer]
%Realtek%      = Realtek, NTx86.5.1, NTamd64

[ControlFlags]
ExcludeFromSelect = *

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
;8101E
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;RTL8131
%RTL8131.DeviceDesc%    = RTL8131.ndi,      PCI\VEN_10EC&DEV_8131&REV_01
%RTL8131.DeviceDesc%    = RTL8131.ndi,      PCI\VEN_10EC&DEV_8131&SUBSYS_813110EC&REV_01

;8102E/8103E
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02

;8104E
%RTL8104.DeviceDesc%    = RTL8104.ndi,     PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104.ndi,     PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8168B
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

;8168D
%RTL8168D.DeviceDesc%   = RTL8168D.ndi,     PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168D.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03

[Realtek.NTx86.5.1]; This section will only be installed by Windows XP
;8101E
%RTL8136.DeviceDesc%	= RTL8136x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;RTL8131
%RTL8131.DeviceDesc%	= RTL8131x.ndi,	    PCI\VEN_10EC&DEV_8131&REV_01
%RTL8131.DeviceDesc%	= RTL8131x.ndi,     PCI\VEN_10EC&DEV_8131&SUBSYS_813110EC&REV_01

;8102E/8103E
%RTL8102.DeviceDesc%	= RTL8102x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02

;8104E
%RTL8104.DeviceDesc%    = RTL8104x.ndi,     PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104x.ndi,     PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8168B
%RTL8168.DeviceDesc%	= RTL8168x.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSx.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

;8168D
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03

[Realtek.NTamd64]; This section will only be installed by Windows XP 64-bit
;8101E
%RTL8136.DeviceDesc%	= RTL8136a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;RTL8131
%RTL8131.DeviceDesc%	= RTL8131a.ndi,	    PCI\VEN_10EC&DEV_8131&REV_01
%RTL8131.DeviceDesc%	= RTL8131a.ndi,     PCI\VEN_10EC&DEV_8131&SUBSYS_813110EC&REV_01

;8102E/8103E
%RTL8102.DeviceDesc%	= RTL8102a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02

;8104E
%RTL8104.DeviceDesc%    = RTL8104a.ndi,     PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104a.ndi,     PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8168B
%RTL8168.DeviceDesc%  	= RTL8168a.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%	= RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSa.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS

;8168D
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
;;RTL8168(98/ME)
[RTL8168.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C(98/ME)
[RTL8168C.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, PowerDownPll.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C ASUS(98/ME)
[RTL8168CASUS.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = WolCap.reg, PowerDownPll.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168D(98/ME)
[RTL8168D.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136(98/ME)
[RTL8136.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136 HP(98/ME)
[RTL8136HP.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = AutoCrossoverDet.reg, WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8131(98/ME)
[RTL8131.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8102E(98/ME)
[RTL8102.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, PowerDownPll.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8104E(98/ME)
[RTL8104.ndi]
DriverVer       = 10/30/2008,708
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, PowerDownPll.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

[Rtlnic.CopyFiles9x]
Rtenic.sys,,,2

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
;;RTL8168(W2K)
[RTL8168.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(W2K)
[RTL8168C.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168C.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(W2K)
[RTL8168CASUS.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168CASUS.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(W2K)
[RTL8168D.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168D.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136(W2K)
[RTL8136.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8136.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(W2K)
[RTL8136HP.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8136HP.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8131(W2K)
[RTL8131.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8131.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(W2K)
[RTL8102.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8102.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(W2K)
[RTL8104.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8104.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtenic.sys,,,2

[RTNicProp.CopyList2K]
RtNicProp32.dll,,,0x10

;;****************************************************************************
;; Windows XP
;;****************************************************************************
;;RTL8168(XP)
[RTL8168x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP)
[RTL8168Cx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168Cx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP)
[RTL8168CASUSx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168CASUSx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP)
[RTL8168Dx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168Dx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP)
[RTL8136x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8136x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136HP(XP)
[RTL8136HPx.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8136HPx.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8131(XP)
[RTL8131x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8131x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP)
[RTL8102x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8102x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(XP)
[RTL8104x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8104x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtenicxp.sys,,,2

[RTNicProp.CopyListXP]
RtNicProp32.dll,,,0x10

;;****************************************************************************
;; Windows XP 64-bit
;;****************************************************************************
;;RTL8168(XP64)
[RTL8168a.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP64)
[RTL8168Ca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168Ca.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP64)
[RTL8168CASUSa.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168CASUSa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP64)
[RTL8168Da.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168Da.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP64)
[RTL8136a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8136a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(XP64)
[RTL8136HPa.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8136HPa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8131(XP64)
[RTL8131a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8131a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP64)
[RTL8102a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8102a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(XP64)
[RTL8104a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg, PowerDownPll.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8104a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[Rtlnic.CopyFilesX64]
Rtenic64.sys,,,2

[RTNicProp.CopyListX64]
RtNicProp64.dll,,,0x10

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8168.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8168"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

[rtl8136.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8136"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; Del parameters
;;****************************************************************************
[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan
HKR,,SuperSwitch
HKR,,PowerDownPll

[TsPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan

;;****************************************************************************
;; common parameters
;;****************************************************************************

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	type,		0, "edit"
HKR,Ndi\params\NetworkAddress,	default,	0, "000000000000"
HKR,Ndi\params\NetworkAddress,	LimitText,	0, "12"
HKR,Ndi\params\NetworkAddress,	UpperCase,	0, "1"
HKR,Ndi\params\NetworkAddress,	Optional,	0, "1"

[Speed.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%
HKR,,DuplexMode,0,"1"

[Speed10_100.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR,,DuplexMode,0,"1"

;[TxDescNumber.reg]
;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"
;HKR,,NumTxDesc,0,"256"

;[RxDescNumber.reg]
;HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
;HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumRxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumRxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumRxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"
;HKR,,NumRxDesc,0,"256"

[68BJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,,Jumboframe,0,"0"

[68CJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "4",        0, %5KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "5",        0, %6KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "6",        0, %7KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "7",        0, %8KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "8",        0, %9KBMTU%
HKR,,Jumboframe,0,"0"

[Flowctrl.reg]
HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, %Disabled%
HKR,Ndi\params\FlowControl\enum, "1",        0, %Enabled%
HKR,,FlowControl,0,"1" 

[S5Wol.reg]
HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[powersavingautophy.reg]
HKR,Ndi\params\AutoLinkDownPhyOff,       ParamDesc,  0, %AutoLinkDownPhyOff%
HKR,Ndi\params\AutoLinkDownPhyOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPhyOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPhyOff,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[WolShutdownLinkSpeed.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "0"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolShutdownLinkSpeedIntel.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "2"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "2",        0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolCap.reg]
HKR, Ndi\params\WolCap,            ParamDesc,  0, %WolCap%
HKR, Ndi\params\WolCap,            type,       0, "enum"
HKR, Ndi\params\WolCap,            default,    0, "3"
HKR, Ndi\params\WolCap\enum,       "0",        0, %None%
HKR, Ndi\params\WolCap\enum,       "1",        0, %PatternMatch%
HKR, Ndi\params\WolCap\enum,       "2",        0, %MagicPacket%
HKR, Ndi\params\WolCap\enum,       "3",        0, %PatternAndMagic%
HKR,,WolCap,0,"3"

[GreenEthernetEnabled.reg]
HKR,Ndi\params\GreenEthernet,      ParamDesc,  0, %GreenEthernet%
HKR,Ndi\params\GreenEthernet,      default,    0, "1"
HKR,Ndi\params\GreenEthernet,      type,       0, "enum"
HKR,Ndi\params\GreenEthernet\enum, "0",        0, %Disabled%
HKR,Ndi\params\GreenEthernet\enum, "1",        0, %Enabled%
HKR,,GreenEthernet,0,"1"

[GreenEthernetDisabled.reg]
HKR,Ndi\params\GreenEthernet,      ParamDesc,  0, %GreenEthernet%
HKR,Ndi\params\GreenEthernet,      default,    0, "0"
HKR,Ndi\params\GreenEthernet,      type,       0, "enum"
HKR,Ndi\params\GreenEthernet\enum, "0",        0, %Disabled%
HKR,Ndi\params\GreenEthernet\enum, "1",        0, %Enabled%
HKR,,GreenEthernet,0,"0"

;[AutoSpeedDown.reg]
;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, %Disabled%
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, %Enabled%
;HKR,,AutoSpeedDown,0,"1"

;[SuperSwitch.reg]
;HKR,,SuperSwitch,0,"0"

[PowerDownPll.reg]
HKR,,PowerDownPll,0,"0"

[ForceMode.reg]
HKR,,ForceMode,0,"0"

[RtNicProp32.reg]
HKR,,EnumPropPages32,,"rtnicprop32.dll,RTNicPropPageProvider"

[RtNicProp64.reg]
HKR,,EnumPropPages32,,"rtnicprop64.dll,RTNicPropPageProvider"

;;****************************************************************************
;; NT parameters
;;****************************************************************************

[OffloadChksum.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\CksOffload\enum,   "1",        0, %RxTxEnabled%
HKR,Ndi\params\CksOffload\enum,   "3",        0, %RxEnabled%
HKR,Ndi\params\CksOffload\enum,   "4",        0, %TxEnabled%
HKR,,CksOffload,0,"1" 

[OffloadLargesend.reg]
HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\Largesend\enum,    "1",        0, %Enabled%
HKR,,Largesend,0,"1" 

[VLanTagging.reg]
HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, %Disabled%
HKR,Ndi\params\Support8021p\enum, "1",        0, %Enabled%
HKR,,Support8021p,0,"0" 

;[VLanID.reg]
;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"
;HKR,,RegVlanid,0,"0" 

;[TxHPQDescNumber.reg]
;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"
;HKR,,NumTxDescHPQ,0,"256" 

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,	ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,	default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,	type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTLE8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic.sys
LoadOrderGroup  = NDIS

[RTLE8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenicxp.sys
LoadOrderGroup  = NDIS

[RTLE8023x64.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023x64"

[rtsntx64.Service]
DisplayName     = %Rtlnicx64.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFilesX64        = 12
Rtlnic.CopyFiles9x         = 11
RTNicProp.CopyList2k       = 11
RTNicProp.CopyListXP       = 11
RTNicProp.CopyListX64      = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtenic.sys	= 1
Rtenicxp.sys	= 1
Rtenic64.sys	= 1
RTNicProp32.dll	= 1
RTNicProp64.dll	= 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN Tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Checksum Offload"
LargesendOffload	= "Large Send Offload"
SpeedDuplexMode		= "Speed & Duplex"
auto_nego		= "Auto Negotiation"
sd10half		= "10 Mbps Half Duplex"
sd10full		= "10 Mbps Full Duplex"
sd100half		= "100 Mbps Half Duplex"
sd100full		= "100 Mbps Full Duplex"
sd1000full		= "1.0 Gbps Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Number of Tx Descriptor"
;RxDescNumber		= "Number of Rx Descriptor"
;TxHPQDescNumber	= "Number of High Priority Tx Descriptor"
FlowControl		= "Flow Control"
;AutoSpeedDown		= "Auto Speed Down"
S5WakeOnLan		= "Shutdown Wake-On-Lan"
10MbFirst               = "10 Mbps First"
100MbFirst              = "100 Mbps First"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "WOL & Shutdown Link Speed"
AutoCrossoverDet        = "Auto Crossover Detection"
Disabled                = "Disabled"
Enabled                 = "Enabled"
TxEnabled               = "Tx Enabled"
RxEnabled               = "Rx Enabled"
RxTxEnabled             = "Rx & Tx Enabled"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Auto Disable PCIe (PowerSaving)"
AutoLinkDownPhyOff      = "Auto Disable PHY (PowerSaving)"
Battery                 = "Enabled, Battery"
AcBattery               = "Enabled, Battery or AC"
GreenEthernet           = "Green Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek RTL8168/8111 PCI-E Gigabit Ethernet NIC"
RTL8168C.DeviceDesc       = "Realtek RTL8168C(P)/8111C(P) PCI-E Gigabit Ethernet NIC"
RTL8168D.DeviceDesc       = "Realtek RTL8168D(P)/8111D(P) PCI-E Gigabit Ethernet NIC"
RTL8136.DeviceDesc        = "Realtek RTL8139/810x Family Fast Ethernet NIC"
RTL8131.DeviceDesc        = "Realtek RTL8131 Family PCI-E Fast Ethernet NIC"
RTL8102.DeviceDesc        = "Realtek RTL8102E/RTL8103E Family PCI-E Fast Ethernet NIC"
RTL8104.DeviceDesc        = "Realtek RTL8104E Family PCI-E Fast Ethernet NIC"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"