
;RTL8168/8111 and RTL8100E  OEMSETUP.INF File:

[netcard]
RTL8168="RTL8168/8111 Family Gigabit Ethernet Adapter",000,ndis,ethernet,real,RTL8168,RTL8168_nif


[RTL8168]
devdir=?:rtend.dos
device=rtend.dos,@devdir\rtend.dos

[RTL8168_nif]
drivername=rtend$
param=Medium,"Medium type ",text,"_Auto,_1000Full,_100Full,_100Half,_10Full,_10Half",_Auto,0x30
param=NETADDRESS,"Network Address",chars,13,"@000000000000",0x02
param=ETHERID,"Node Address",chars,13,"@000000000000",0x02
param=BusNo ,"Adpater's Bus Number",int,"0,255,1",0,0x32
param=DeviceNo ,"Adpater's Device Number",int,"0,31,1",0,0x32
